|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date of Testing** | | 02-09-2022 | | **COA No:** | | | | COA046 | | | |
| **Material Name** | | PEEK | | **Batch/Lot No. (If Available)** | | | | B005644 | | | |
| **Material Quantity** | | 28 | | **Any reference** | | | |  | | | |
| **Manufacturing date** | | 27-08-2022 | | **Expiry date** | | | | 04-09-2022 | | | |
| **Sr. No.** | **Testing Parameter** | **Testing Method** | **Acceptance Criteria** | | **Sampling Method** | **Observations** | | | | | **Remarks** |
| **1** | **2** | | **3** | **4** |
|  | Width | length gauge | 7.0±0.1 | | Refer SOP for inspection | 6.93 | 7.05 | | 7.0 | 7.1 |  |
|  | Slot size | length gauge | 2.0±0.1 | | 1.97 | 1.96 | | 2.1 | 2.08 |  |
|  | Shape | Visual | Similar | | Similar | Similar | | Similar | Similar |  |
|  | Thickness | length gauge | 1.0±0.01 | | 1.0 | 1.0 | | 0.99 | 1.01 |  |
|  | Length | length gauge | 5.0±0.01 | | 5.01 | 4.99 | | 5.0 | 5.01 |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| √ | **Approved** | **Comments/Instructions:** | **Inspected By** | Pankaj |
| × | **Rejected** |  |
| **Verified and Approved By** | Arvind |