|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date of Testing** | | 10-09-2022 | | **COA No:** | | | | COA050 | | | |
| **Material Name** | | SS | | **Batch/Lot No. (If Available)** | | | | Boo5680 | | | |
| **Material Quantity** | | 75 | | **Any reference** | | | |  | | | |
| **Manufacturing date** | | 04-09-2022 | | **Expiry date** | | | | 12-09-2022 | | | |
| **Sr. No.** | **Testing Parameter** | **Testing Method** | **Acceptance Criteria** | | **Sampling Method** | **Observations** | | | | | **Remarks** |
| **1** | **2** | | **3** | **4** |
|  | Thickness | Vernier caliper | 10.0±0.1 | | Refer SOP for inspection | 9.92 | 9.91 | | 9.9 | 9.93 |  |
|  | Width | Vernier caliper | 5.0±0.1 | | 5.06 | 4.99 | | 5.09 | 4.99 |  |
|  | Length | Vernier caliper | 30.0±1.0 | | 29.34 | 30.5 | | 29.24 | 29.16 |  |
|  | Hole size | Vernier caliper | 2.0±0.05 | | 2.0 | 2.04 | | 1.95 | 2.0 |  |
|  | Shape | Visual | Similar | | Similar | Similar | | Similar | Similar |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| √ | **Approved** | **Comments/Instructions:** | **Inspected By** | Sumit |
| × | **Rejected** |  |
| **Verified and Approved By** | Rajiv |